|  |  |
| --- | --- |
| **Name:** |  |
| **Date:** |  |
| **TASK:** | **Pole Pruner & Pole Hedger** | **Stage 1 of 2 stages in task** |
| TA: | Start - 2 Stroke |
| **Name of Assessor:** |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| A Skill level of**...A...B...C...D...E...**Indicate level using underpinning work skill guide**Steps requiring skill level : List by step number**

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |  |  |  |  |

**Office use only** |

|  |  |  |  |
| --- | --- | --- | --- |
|  | **Assistance coding:**0=no assistance/fully independent1=indirect verbal prompts/instructions2=gestural prompts3=direct verbal prompts/instructions4=model style prompting5=physical prompting MINIMAL6=physical prompting FULL assistance7=not complaint/failed taskN/A=not applicable  | OBSERVATION DATES  | Associated: * Safe Work Procedure
* Safety Data Sheet

OHS requirements* Safety Glasses
* Gloves - tech/riggers
* Ear muffs
* Steel capped boots
* Work clothing
* Safety helmet
* Sun protection
 |
| 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8 | 9 | 10 | 11 | 12 | 13 |
|  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | **Staff initials**: |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |
|  | STEPS  | ASSISTANCE REQURED |
| **1** | Use of OHS requirements |  |  |  |  |  |  |  |  |  |  |  |  |  | SUPERVISOR:* Pre – safety checks
* Worker supervision is required when refuelling
 |
| **2** | *Refuelling procedure GRF-02* |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **3** | Remove unrequired attachment & attach required extension  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **4** | *2 Stroke starting procedure GRF-23* |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **5** | Need the trigger action on, to hold the throttle on, to start the machine |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **6** | Before starting make sure chain/hedger is clear of the ground. Use the pull start chord to get the pruner pole going. |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **7** | *See operation of Pole Pruner/Hedger stage 2 of 2 task assessment* |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **8** | Shut off the engine before setting the pruner down |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **9** |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **10** |  |  |  |  |  |  |  |  |  |  |  |  |  |  |

**Comments:**

|  |
| --- |
|  |